"Base-Width"= 420

"Base-Width-Medium"= 520

"Base-Height"= 320

"Support-Rod-Diameter"= 16

"Support-Rod-X-Offset"= 35

"Support-Rod-Y-Offset"= 35

"Base-Thickness"= 5

"Base-Depth"= 82

"D2@Sketch1"="Base-Width"

"D1@Sketch1"="Base-Height"

"Corner-Radius-Major"= "Support-Rod-Diameter"

"D1@Major-Fillet" = "Corner-Radius-Major"

"D1@Sketch8" = "Base-Height" - "Support-Rod-Y-Offset" + 12

"D2@Sketch8"= "Base-Width" - ( "Support-Rod-X-Offset" ) + 12

"Cutout-Horizontal"= "Base-Width" * 0.8

"Cutout-Vertical"= "Base-Height" * 0.6

"Outer-Support-Bore-Diameter"= 6.1

"D2@Sketch6"="Cutout-Horizontal"

"D1@Sketch7"="Cutout-Vertical"

"Inner-Support-Bore-Diameter"= 8.2

"Cutout-Depth"= 20

"D1@Sketch6"="Cutout-Depth"

"D2@Sketch7"="Cutout-Depth"

"D4@Sketch1"="Inner-Support-Bore-Diameter"

"D1@Minor-Fillets"="Corner-Radius-Major" / 2

